I have a question about the NTP proposal:

* There appears to be an inconsistency between Application Note 35 in NDcPP and FCS\_NTP\_EXT.1.4 of the proposed requirement.

The NTP proposal for FCS\_NTP\_EXT.1.4 states:

   "The TSF shall support configuration of ***at least three (3) NTP time sources***".

This reads as though the intention is to mandate the use of a minimum of 3 NTP time sources.  However, NDcPP Application Note 35 (para 1) states:

   "The TOE depends on external time and date information, either provided manually by the Security Administrator or through the use of ***one or more*** external time sources like NTP servers".

Is it the subgroup's intention that Application Note 35 should be updated to state "The TOE depends on external time and date information, either provided manually by the Security Administrator or through the use of ~~one~~ three or more external time sources like NTP servers" ?

**NTP Subgroup response:** The number of NTP servers in the proposed requirement is the capability of the TOE. The use of three time sources is not a mandate. The application note (35) will be updated to state the use of three time sources is not mandated.